| Wireshark 4.7.0 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
_packet_info Struct Reference
Packet Data and Metadata

## Public Attributes
const char * | current_proto
struct epan_column_info * | cinfo
uint32_t | presence_flags
uint32_t | num
nstime_t | abs_ts
nstime_t | rel_ts
nstime_t | rel_cap_ts
bool | rel_cap_ts_present
frame_data * | fd
union wtap_pseudo_header * | pseudo_header
wtap_rec * | rec
GSList * | data_src
address | dl_src
address | dl_dst
address | net_src
address | net_dst
address | src
address | dst
uint32_t | vlan_id
const char * | noreassembly_reason
bool | fragmented
struct { |
uint32_t in_error_pkt: 1 |
uint32_t in_gre_pkt: 1 |
} | flags |
uint32_t | expert_severity
port_type | ptype
uint32_t | srcport
uint32_t | destport
uint32_t | match_uint
const char * | match_string
bool | use_conv_addr_port_endpoints
struct conversation_addr_port_endpoints * | conv_addr_port_endpoints
struct conversation_element * | conv_elements
uint16_t | can_desegment
uint16_t | saved_can_desegment
int | desegment_offset
uint32_t | desegment_len
uint16_t | want_pdu_tracking
uint32_t | bytes_until_next_pdu
int | p2p_dir
GHashTable * | private_table
wmem_list_t * | layers
wmem_map_t * | proto_layers
uint8_t | curr_layer_num
uint8_t | curr_proto_layer_num
uint16_t | link_number
uint16_t | clnp_srcref
uint16_t | clnp_dstref
int | link_dir
int16_t | src_win_scale
int16_t | dst_win_scale
GSList * | proto_data
GSList * | frame_end_routines
wmem_allocator_t * | pool
struct epan_session * | epan
const char * | heur_list_name
int | dissection_depth
uint32_t | stream_id
uint32_t | track_ctype
const char * | user_name

## Member Data Documentation

## ◆ abs_ts

nstime_t _packet_info::abs_ts

Packet absolute timestamp

## ◆ bytes_until_next_pdu

uint32_t _packet_info::bytes_until_next_pdu

Number of bytes until the next PDU starts beyond the next segment

## ◆ can_desegment

uint16_t _packet_info::can_desegment

>0 if this segment could be desegmented. A dissector that can offer this API (e.g. TCP) sets can_desegment=2, then can_desegment is decremented by 1 each time we pass to the next subdissector. Thus only the dissector immediately above the protocol which sets the flag can use it

## ◆ cinfo

struct epan_column_info* _packet_info::cinfo

Column formatting information

## ◆ clnp_dstref

uint16_t _packet_info::clnp_dstref

CLNP/COTP destination reference (cannot use dstport to avoid confusion with TPKT)

## ◆ clnp_srcref

uint16_t _packet_info::clnp_srcref

CLNP/COTP source reference (cannot use srcport to avoid confusion with TPKT)

## ◆ conv_addr_port_endpoints

struct conversation_addr_port_endpoints* _packet_info::conv_addr_port_endpoints

Address+port conversation data, including wildcarding

## ◆ conv_elements

struct conversation_element* _packet_info::conv_elements

Arbitrary conversation identifier (cannot be wildcarded)

## ◆ curr_layer_num

uint8_t _packet_info::curr_layer_num

Current "depth" or layer number in the current frame

## ◆ curr_proto_layer_num

uint8_t _packet_info::curr_proto_layer_num

Current "depth" or layer number for this dissector in the current frame

## ◆ current_proto

const char* _packet_info::current_proto

Name of protocol currently being dissected

## ◆ data_src

GSList* _packet_info::data_src

Frame data sources

## ◆ desegment_len

uint32_t _packet_info::desegment_len

requested desegmentation additional length or DESEGMENT_ONE_MORE_SEGMENT: Desegment one more full segment (warning! only partially implemented) DESEGMENT_UNTIL_FIN: Desegment all data for this tcp session until the FIN segment.

## ◆ desegment_offset

int _packet_info::desegment_offset

Offset to data needing desegmentation

## ◆ destport

uint32_t _packet_info::destport

Destination port

## ◆ dissection_depth

int _packet_info::dissection_depth

Current "depth" or layer number in the current frame

## ◆ dl_dst

address _packet_info::dl_dst

Link-layer destination address

## ◆ dl_src

address _packet_info::dl_src

Link-layer source address

## ◆ dst

address _packet_info::dst

Destination address (network if present, else DL)

## ◆ dst_win_scale

int16_t _packet_info::dst_win_scale

Rcv.Wind.Shift dst applies when sending segments; -1 unknown; -2 disabled

## ◆ epan

struct epan_session* _packet_info::epan

Pointer to the current epan session context

## ◆ expert_severity

uint32_t _packet_info::expert_severity

Highest expert severity level

## ◆ fd

frame_data* _packet_info::fd

Frame metadata and indexing information

## ◆ fragmented

bool _packet_info::fragmented

True if the protocol is a fragment

## ◆ frame_end_routines

GSList* _packet_info::frame_end_routines

List of routines to execute after frame dissection

## ◆ heur_list_name

const char* _packet_info::heur_list_name

Name of heuristic list if packet is being heuristically dissected

## ◆ in_error_pkt

uint32_t _packet_info::in_error_pkt

True if inside an error packet (e.g., ICMP, CLNP)

## ◆ in_gre_pkt

uint32_t _packet_info::in_gre_pkt

True if encapsulated inside a GRE packet

## ◆ layers

wmem_list_t* _packet_info::layers

List of protocol layers

## ◆ link_dir

int _packet_info::link_dir

Link direction (e.g., 3GPP uplink or downlink)

## ◆ link_number

uint16_t _packet_info::link_number

Link-layer interface index

## ◆ match_string

const char* _packet_info::match_string

Matched string for calling subdissector from a table

## ◆ match_uint

uint32_t _packet_info::match_uint

Matched uint for calling subdissector from a table

## ◆ net_dst

address _packet_info::net_dst

Network-layer destination address

## ◆ net_src

address _packet_info::net_src

Network-layer source address

## ◆ noreassembly_reason

const char* _packet_info::noreassembly_reason

Reason why reassembly was not performed, if any

## ◆ num

uint32_t _packet_info::num

Frame number

## ◆ p2p_dir

int _packet_info::p2p_dir

Packet was captured as an outbound (P2P_DIR_SENT) inbound (P2P_DIR_RECV) unknown (P2P_DIR_UNKNOWN)

## ◆ pool

wmem_allocator_t* _packet_info::pool

Memory pool scoped to this pinfo

## ◆ presence_flags

uint32_t _packet_info::presence_flags

Presence flags for some items

## ◆ private_table

GHashTable* _packet_info::private_table

Hash table passed between dissectors

## ◆ proto_data

GSList* _packet_info::proto_data

Per-packet protocol data

## ◆ proto_layers

wmem_map_t* _packet_info::proto_layers

Map from proto_id to curr_proto_layer_num

## ◆ pseudo_header

union wtap_pseudo_header* _packet_info::pseudo_header

Capture-specific pseudo header (e.g., Ethernet, 802.11)

## ◆ ptype

port_type _packet_info::ptype

Type of the srcport and destport

## ◆ rec

wtap_rec* _packet_info::rec

Record metadata

## ◆ rel_cap_ts

nstime_t _packet_info::rel_cap_ts

Relative timestamp from capture start (may be negative for broken files)

## ◆ rel_cap_ts_present

bool _packet_info::rel_cap_ts_present

True if relative capture timestamp is valid

## ◆ rel_ts

nstime_t _packet_info::rel_ts

Relative timestamp (can be negative)

## ◆ saved_can_desegment

uint16_t _packet_info::saved_can_desegment

Value of can_desegment before current dissector was called. Supplied so that dissectors for proxy protocols such as SOCKS can restore it, allowing the dissectors that they call to use the TCP dissector's desegmentation (SOCKS just retransmits TCP segments once it's finished setting things up, so the TCP desegmentor can desegment its payload).

## ◆ src

address _packet_info::src

Source address (network if present, else DL)

## ◆ src_win_scale

int16_t _packet_info::src_win_scale

Rcv.Wind.Shift src applies when sending segments; -1 unknown; -2 disabled

## ◆ srcport

uint32_t _packet_info::srcport

Source port

## ◆ stream_id

uint32_t _packet_info::stream_id

Conversation stream ID of the highest protocol

## ◆ track_ctype

uint32_t _packet_info::track_ctype

Tracks the conversation type for these protocols subscribing to an error packet follow-up. Typically transport protocols such as UDP or TCP are likely to be followed up by ICMP.

## ◆ use_conv_addr_port_endpoints

bool _packet_info::use_conv_addr_port_endpoints

True if address/port endpoints should be used for conversations

## ◆ user_name

const char* _packet_info::user_name

Text user name

## ◆ vlan_id

uint32_t _packet_info::vlan_id

First encountered VLAN ID if present, else 0

## ◆ want_pdu_tracking

uint16_t _packet_info::want_pdu_tracking

>0 if the subdissector has specified a value in 'bytes_until_next_pdu'. When a dissector detects that the next PDU will start beyond the start of the next segment, it can set this value to 2 and 'bytes_until_next_pdu' to the number of bytes beyond the next segment where the next PDU starts.

If the protocol dissector below this one is capable of PDU tracking it can use this hint to detect PDUs that starts unaligned to the segment boundaries. The TCP dissector is using this hint from (some) protocols to detect when a new PDU starts in the middle of a tcp segment.

There is intelligence in the glue between dissector layers to make sure that this request is only passed down to the protocol immediately below the current one and not any further.

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/epan/packet_info.h