| Wireshark 4.7.0 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
packet-sflow.h
1/* packet-sflow.h
2 * sFlow v5 dissection implemented according to the specifications
3 * at http://www.sflow.org/sflow_version_5.txt
4 *
5 * Wireshark - Network traffic analyzer
6 * By Gerald Combs <gerald@wireshark.org>
7 * Copyright 1998 Gerald Combs
8 *
9 * SPDX-License-Identifier: GPL-2.0-or-later
10 */
11
12#ifndef __PACKET_SFLOW_H__
13#define __PACKET_SFLOW_H__
14
15#define SFLOW_245_HEADER_ETHERNET 1
16#define SFLOW_245_HEADER_TOKENBUS 2
17#define SFLOW_245_HEADER_TOKENRING 3
18#define SFLOW_245_HEADER_FDDI 4
19#define SFLOW_245_HEADER_FRAME_RELAY 5
20#define SFLOW_245_HEADER_X25 6
21#define SFLOW_245_HEADER_PPP 7
22
23/* We don't have an SMDS dissector yet
24 *
25 * Switched multimegabit data service (SMDS) was a connectionless service
26 * used to connect LANs, MANs and WANs to exchange data. SMDS was based on
27 * the IEEE 802.6 DQDB standard. SMDS fragmented its datagrams into smaller
28 * "cells" for transport, and can be viewed as a technological precursor of ATM.
29 */
30#define SFLOW_245_HEADER_SMDS 8
31
32/*
33 * No AAL5 (ATM Adaptation Layer 5) dissector available.
34 * What does the packet look like? An AAL5 PDU? Where
35 * do the VPI/VCI pair appear, if anywhere?
36 */
37#define SFLOW_245_HEADER_AAL5 9
38#define SFLOW_245_HEADER_AAL5_IP 10
39
40#define SFLOW_245_HEADER_IPv4 11
41#define SFLOW_245_HEADER_IPv6 12
42#define SFLOW_245_HEADER_MPLS 13
43
44/* wireshark does not have POS dissector yet */
45#define SFLOW_5_HEADER_POS 14
46
47#define SFLOW_5_HEADER_80211_MAC 15
48
49/* XXX - No handles for these, need to be converted into "dissectors" */
50#define SFLOW_5_HEADER_80211_AMPDU 16 /* "wlan_aggregate" */
51#define SFLOW_5_HEADER_80211_AMSDU_SUBFRAME 17
52
53#endif