| Wireshark 4.7.0 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
packet-darwin-droptap-msg.h
1/* packet-darwin-droptap-msg.h
2 * Decoding of Darwin droptap message code.
3 *
4 * Copyright (c) 2024-2025 Apple Inc. All rights reserved.
5 * Licensed under the terms of the MIT License.
6 *
7 * Wireshark - Network traffic analyzer
8 * By Gerald Combs <gerald@wireshark.org>
9 * Copyright 1998 Gerald Combs
10 *
11 * SPDX-License-Identifier: MIT
12 */
13#ifndef PACKET_DARWIN_DROPTAP_MSG_H
14#define PACKET_DARWIN_DROPTAP_MSG_H
15
16#include <stdint.h>
17
18/*
19 * Drop Reason is a 32-bit encoding of drop code, domain, and component.
20 *
21 * Drop Reason
22 * +----+----+--------+----------------+
23 * | 4 | 4 | 8 | 16 |
24 * +----+----+--------+----------------+
25 * ^ ^ ^ ^
26 * | | | Drop Code
27 * | | Domain
28 * | Component
29 * Reserved
30 *
31 * [ 15:0] Drop Code: Specific reason why the drop happened (e.g. AQM full)
32 * [23:16] Domain : Which domain the drop happened (e.g. Flowswitch, TCP, IP)
33 * [27:24] Component: Which component the drop happened (e.g. Skywalk, BSD, driver)
34 * [31:28] Reserved : Reserved for future use
35 *
36 * This code is structured similarly to the implementation in the Darwin xnu kernel
37 * to allow easier updates as the Darwin codebase evolves.
38 */
39
40#define DROP_COMPONENT_MASK 0x0f000000
41#define DROP_COMPONENT_OFFSET 24
42#define DROP_COMPONENT_MAX 0x0f
43#define DROP_DOMAIN_MASK 0x00ff0000
44#define DROP_DOMAIN_OFFSET 16
45#define DROP_DOMAIN_MAX 0xff
46#define DROP_CODE_MASK 0x0000ffff
47#define DROP_CODE_OFFSET 0
48#define DROP_CODE_MAX 0xffff
49
50/* 32-bit Drop Reason */
51#define DROP_REASON(component, domain, code) \
52 (((unsigned)((component) & DROP_COMPONENT_MAX) << DROP_COMPONENT_OFFSET) | \
53 ((unsigned)((domain) & DROP_DOMAIN_MAX) << DROP_DOMAIN_OFFSET) | \
54 ((unsigned)((code) & DROP_CODE_MAX) << DROP_CODE_OFFSET))
55
56/* All components */
57#define DROPTAP_SKYWALK 1
58#define DROPTAP_BSD 2
60/* All domains for the Skywalk (user-space networking) component */
61#define DROPTAP_FSW 1
62#define DROPTAP_NETIF 2
63#define _DROPTAP_PAD_3 3
64#define _DROPTAP_PAD_4 4
65#define DROPTAP_AQM 5
67/* All domains for the BSD component */
68#define DROPTAP_TCP 1
69#define DROPTAP_UDP 2
70#define DROPTAP_IP 3
71#define DROPTAP_SOCK 4
72#define DROPTAP_DLIL 5
73#define DROPTAP_IPSEC 6
74#define DROPTAP_IP6 7
75#define DROPTAP_MPTCP 8
76#define DROPTAP_PF 9
77#define DROPTAP_BRIDGE 10
79#define DROPTAP_UNSPEC 0
82#define DARWIN_DROP_REASON_LIST(X) \
83 X(DROP_REASON_UNSPECIFIED, DROPTAP_UNSPEC, DROPTAP_UNSPEC, DROPTAP_UNSPEC, "Drop reason not specified") \
84 /* Skywalk component */ \
85 X(DROP_REASON_FSW_PP_ALLOC_FAILED, DROPTAP_SKYWALK, DROPTAP_FSW, 1, "Flowswitch packet alloc failed") \
86 X(DROP_REASON_RX_DST_RING_FULL, DROPTAP_SKYWALK, DROPTAP_FSW, 2, "Flowswitch Rx destination ring full") \
87 X(DROP_REASON_FSW_QUIESCED, DROPTAP_SKYWALK, DROPTAP_FSW, 3, "Flowswitch detached") \
88 X(DROP_REASON_FSW_IFNET_NOT_ATTACHED, DROPTAP_SKYWALK, DROPTAP_FSW, 4, "Flowswitch ifnet not attached") \
89 X(DROP_REASON_FSW_DEMUX_FAILED, DROPTAP_SKYWALK, DROPTAP_FSW, 5, "Flowswitch demux error") \
90 X(DROP_REASON_FSW_TX_DEVPORT_NOT_ATTACHED, DROPTAP_SKYWALK, DROPTAP_FSW, 6, "Flowswitch destination nexus port inactive") \
91 X(DROP_REASON_FSW_TX_FLOW_EXTRACT_FAILED, DROPTAP_SKYWALK, DROPTAP_FSW, 7, "Flowswitch flow extract error") \
92 X(DROP_REASON_FSW_TX_FRAG_BAD_CONT, DROPTAP_SKYWALK, DROPTAP_FSW, 8, "Flowswitch invalid continuation fragment") \
93 X(DROP_REASON_FSW_TX_FLOW_NOT_FOUND, DROPTAP_SKYWALK, DROPTAP_FSW, 9, "Flowswitch flow lookup failed") \
94 X(DROP_REASON_FSW_TX_RESOLV_PENDING, DROPTAP_SKYWALK, DROPTAP_FSW, 10, "Flowswitch resolution pending") \
95 X(DROP_REASON_FSW_TX_RESOLV_FAILED, DROPTAP_SKYWALK, DROPTAP_FSW, 11, "Flowswitch resolution failed") \
96 X(DROP_REASON_FSW_FLOW_NONVIABLE, DROPTAP_SKYWALK, DROPTAP_FSW, 12, "Flowswitch flow not viable") \
97 X(DROP_REASON_FSW_RX_RING_NOT_FOUND, DROPTAP_SKYWALK, DROPTAP_FSW, 13, "Flowswitch Rx ring not found") \
98 X(DROP_REASON_FSW_RX_PKT_NOT_FINALIZED, DROPTAP_SKYWALK, DROPTAP_FSW, 14, "Flowswitch packet not finalized") \
99 X(DROP_REASON_FSW_FLOW_TRACK_ERR, DROPTAP_SKYWALK, DROPTAP_FSW, 15, "Flowswitch flow tracker error") \
100 X(DROP_REASON_FSW_PKT_COPY_FAILED, DROPTAP_SKYWALK, DROPTAP_FSW, 16, "Flowswitch packet copy failed") \
101 X(DROP_REASON_FSW_GSO_FAILED, DROPTAP_SKYWALK, DROPTAP_FSW, 17, "Flowswitch GSO failed") \
102 X(DROP_REASON_FSW_GSO_NOMEM_PKT, DROPTAP_SKYWALK, DROPTAP_FSW, 18, "Flowswitch GSO not enough packet memory") \
103 X(DROP_REASON_FSW_GSO_NOMEM_MBUF, DROPTAP_SKYWALK, DROPTAP_FSW, 19, "Flowswitch GSO not enough mbuf memory") \
104 X(DROP_REASON_FSW_DST_NXPORT_INVALID, DROPTAP_SKYWALK, DROPTAP_FSW, 20, "Flowswitch dst nexus port invalid") \
105 X(DROP_REASON_AQM_FULL, DROPTAP_SKYWALK, DROPTAP_AQM, 1, "AQM full") \
106 X(DROP_REASON_AQM_COMPRESSED, DROPTAP_SKYWALK, DROPTAP_AQM, 2, "AQM compressed") \
107 X(DROP_REASON_AQM_BK_SYS_THROTTLED, DROPTAP_SKYWALK, DROPTAP_AQM, 3, "AQM BK_SYS throttled") \
108 X(DROP_REASON_AQM_PURGE_FLOW, DROPTAP_SKYWALK, DROPTAP_AQM, 4, "AQM purge flow") \
109 X(DROP_REASON_AQM_DROP, DROPTAP_SKYWALK, DROPTAP_AQM, 5, "AQM drop") \
110 X(DROP_REASON_AQM_HIGH_DELAY, DROPTAP_SKYWALK, DROPTAP_AQM, 6, "AQM drop due to high delay") \
111 /* Socket */ \
112 X(DROP_REASON_FULL_SOCK_RCVBUF, DROPTAP_BSD, DROPTAP_SOCK, 1, "Socket receive buffer full") \
113 /* DLIL */ \
114 X(DROP_REASON_DLIL_BURST_LIMIT, DROPTAP_BSD, DROPTAP_DLIL, 1, "DLIL burst limit exceeded") \
115 X(DROP_REASON_DLIL_ENQUEUE_INVALID, DROPTAP_BSD, DROPTAP_DLIL, 2, "DLIL enqueue invalid") \
116 X(DROP_REASON_DLIL_ENQUEUE_IF_NOT_ATTACHED, DROPTAP_BSD, DROPTAP_DLIL, 3, "DLIL enqueue interface not fully attached") \
117 X(DROP_REASON_DLIL_ENQUEUE_IF_NOT_UP, DROPTAP_BSD, DROPTAP_DLIL, 4, "DLIL enqueue interface not up") \
118 X(DROP_REASON_DLIL_IF_FILTER, DROPTAP_BSD, DROPTAP_DLIL, 5, "DLIL interface filter") \
119 X(DROP_REASON_DLIL_IF_DATAMOV_BEGIN, DROPTAP_BSD, DROPTAP_DLIL, 6, "DLIL interface datamove begin") \
120 X(DROP_REASON_DLIL_CLAT64, DROPTAP_BSD, DROPTAP_DLIL, 7, "DLIL CLAT46") \
121 X(DROP_REASON_DLIL_PROMISC, DROPTAP_BSD, DROPTAP_DLIL, 8, "DLIL promiscuous") \
122 X(DROP_REASON_DLIL_NO_PROTO, DROPTAP_BSD, DROPTAP_DLIL, 9, "DLIL no protocol") \
123 X(DROP_REASON_DLIL_PRE_OUTPUT, DROPTAP_BSD, DROPTAP_DLIL, 10, "DLIL pre output") \
124 X(DROP_REASON_DLIL_IF_FRAMER, DROPTAP_BSD, DROPTAP_DLIL, 11, "DLIL interface framer") \
125 X(DROP_REASON_DLIL_TSO_NOT_OK, DROPTAP_BSD, DROPTAP_DLIL, 12, "DLIL interface TSO not OK") \
126 /* MPTCP */ \
127 X(DROP_REASON_MPTCP_INPUT_MALFORMED, DROPTAP_BSD, DROPTAP_MPTCP,1, "MPTCP input packet malformed") \
128 X(DROP_REASON_MPTCP_REASSEMBLY_ALLOC, DROPTAP_BSD, DROPTAP_MPTCP,2, "MPTCP reassembly allocation") \
129 /* PF */ \
130 X(DROP_REASON_PF_UNSPECIFIED, DROPTAP_BSD, DROPTAP_PF, 1, "PF unspecified reason") \
131 X(DROP_REASON_PF_UNDERSIZED, DROPTAP_BSD, DROPTAP_PF, 2, "PF undersized") \
132 X(DROP_REASON_PF_NO_ROUTE, DROPTAP_BSD, DROPTAP_PF, 3, "PF no route") \
133 X(DROP_REASON_PF_NULL_IFP, DROPTAP_BSD, DROPTAP_PF, 4, "PF NULL ifp") \
134 X(DROP_REASON_PF_NO_TSO, DROPTAP_BSD, DROPTAP_PF, 5, "PF No TSO?") \
135 X(DROP_REASON_PF_CANNOT_FRAGMENT, DROPTAP_BSD, DROPTAP_PF, 6, "PF Cannot fragment") \
136 X(DROP_REASON_PF_OVERLAPPING_FRAGMENT, DROPTAP_BSD, DROPTAP_PF, 7, "PF overlapping fragment") \
137 X(DROP_REASON_PF_BAD_FRAGMENT, DROPTAP_BSD, DROPTAP_PF, 8, "PF overlapping fragment") \
138 X(DROP_REASON_PF_MEM_ALLOC, DROPTAP_BSD, DROPTAP_PF, 9, "PF memory allocation") \
139 X(DROP_REASON_PF_DROP, DROPTAP_BSD, DROPTAP_PF, 10, "PF drop") \
140 /* BRIDGE */ \
141 X(DROP_REASON_BRIDGE_UNSPECIFIED, DROPTAP_BSD, DROPTAP_BRIDGE, 1, "Bridge unspecified reason") \
142 X(DROP_REASON_BRIDGE_CHECKSUM, DROPTAP_BSD, DROPTAP_BRIDGE, 2, "Bridge checksum") \
143 X(DROP_REASON_BRIDGE_NOT_RUNNING, DROPTAP_BSD, DROPTAP_BRIDGE, 3, "Bridge not running") \
144 X(DROP_REASON_BRIDGE_PRIVATE_SEGMENT, DROPTAP_BSD, DROPTAP_BRIDGE, 4, "Bridge private segment") \
145 X(DROP_REASON_BRIDGE_NO_PROTO, DROPTAP_BSD, DROPTAP_BRIDGE, 5, "Bridge unknown protocol") \
146 X(DROP_REASON_BRIDGE_BAD_PROTO, DROPTAP_BSD, DROPTAP_BRIDGE, 6, "Bridge bad protocol") \
147 X(DROP_REASON_BRIDGE_MAC_NAT_FAILURE, DROPTAP_BSD, DROPTAP_BRIDGE, 7, "Bridge NAT failure") \
148 X(DROP_REASON_BRIDGE_HOST_FILTER, DROPTAP_BSD, DROPTAP_BRIDGE, 8, "Bridge host filter") \
149 X(DROP_REASON_BRIDGE_HWASSIST, DROPTAP_BSD, DROPTAP_BRIDGE, 9, "Bridge HW assisst") \
150 X(DROP_REASON_BRIDGE_NOREF, DROPTAP_BSD, DROPTAP_BRIDGE, 10, "Bridge noref") \
151 X(DROP_REASON_BRIDGE_PF, DROPTAP_BSD, DROPTAP_BRIDGE, 11, "Bridge PF") \
152 X(DROP_REASON_BRIDGE_LOOP, DROPTAP_BSD, DROPTAP_BRIDGE, 12, "Bridge loop") \
153 X(DROP_REASON_BRIDGE_NOT_A_MEMBER, DROPTAP_BSD, DROPTAP_BRIDGE, 13, "Bridge not a member") \
154 /* TCP */ \
155 X(DROP_REASON_TCP_RST, DROPTAP_BSD, DROPTAP_TCP, 1, "TCP connection reset") \
156 X(DROP_REASON_TCP_REASSEMBLY_ALLOC, DROPTAP_BSD, DROPTAP_TCP, 2, "TCP reassembly allocation") \
157 X(DROP_REASON_TCP_NECP, DROPTAP_BSD, DROPTAP_TCP, 3, "TCP NECP not allowed") \
158 X(DROP_REASON_TCP_PKT_UNSENT, DROPTAP_BSD, DROPTAP_TCP, 4, "TCP unsent packet") \
159 X(DROP_REASON_TCP_SRC_ADDR_NOT_AVAIL, DROPTAP_BSD, DROPTAP_TCP, 5, "TCP source address not available") \
160 X(DROP_REASON_TCP_REASS_OVERFLOW, DROPTAP_BSD, DROPTAP_TCP, 6, "TCP reassembly queue overflow") \
161 X(DROP_REASON_TCP_CHECKSUM_INCORRECT, DROPTAP_BSD, DROPTAP_TCP, 7, "TCP checksum incorrect") \
162 X(DROP_REASON_TCP_SRC_ADDR_UNSPECIFIED, DROPTAP_BSD, DROPTAP_TCP, 8, "TCP source address unspecified") \
163 X(DROP_REASON_TCP_OFFSET_INCORRECT, DROPTAP_BSD, DROPTAP_TCP, 9, "TCP offset incorrect") \
164 X(DROP_REASON_TCP_SYN_FIN, DROPTAP_BSD, DROPTAP_TCP, 10, "TCP SYN with FIN") \
165 X(DROP_REASON_TCP_NO_SOCK, DROPTAP_BSD, DROPTAP_TCP, 11, "TCP no socket") \
166 X(DROP_REASON_TCP_PCB_MISMATCH, DROPTAP_BSD, DROPTAP_TCP, 12, "TCP protocol control block mismatch") \
167 X(DROP_REASON_TCP_NO_PCB, DROPTAP_BSD, DROPTAP_TCP, 13, "TCP no protocol control block") \
168 X(DROP_REASON_TCP_CLOSED, DROPTAP_BSD, DROPTAP_TCP, 14, "TCP state CLOSED") \
169 X(DROP_REASON_TCP_FLAGS_INCORRECT, DROPTAP_BSD, DROPTAP_TCP, 15, "TCP flags incorrect") \
170 X(DROP_REASON_TCP_LISTENER_CLOSING, DROPTAP_BSD, DROPTAP_TCP, 16, "TCP listener closing") \
171 X(DROP_REASON_TCP_SYN_RST, DROPTAP_BSD, DROPTAP_TCP, 17, "TCP SYN with RST") \
172 X(DROP_REASON_TCP_SYN_ACK_LISTENER, DROPTAP_BSD, DROPTAP_TCP, 18, "TCP SYN with ACK for listener") \
173 X(DROP_REASON_TCP_LISTENER_NO_SYN, DROPTAP_BSD, DROPTAP_TCP, 19, "TCP no SYN for listener") \
174 X(DROP_REASON_TCP_SAME_PORT, DROPTAP_BSD, DROPTAP_TCP, 20, "TCP same source and destination ports") \
175 X(DROP_REASON_TCP_BCAST_MCAST, DROPTAP_BSD, DROPTAP_TCP, 21, "TCP address not unicast") \
176 X(DROP_REASON_TCP_DEPRECATED_ADDR, DROPTAP_BSD, DROPTAP_TCP, 22, "TCP address deprecated") \
177 X(DROP_REASON_TCP_LISTENER_DROP, DROPTAP_BSD, DROPTAP_TCP, 23, "TCP listener drop") \
178 X(DROP_REASON_TCP_PCB_HASH_FAILED, DROPTAP_BSD, DROPTAP_TCP, 24, "TCP protocol control block hash") \
179 X(DROP_REASON_TCP_CONTENT_FILTER_ATTACH, DROPTAP_BSD, DROPTAP_TCP, 25, "TCP control filter attach") \
180 X(DROP_REASON_TCP_BIND_IN_PROGRESS, DROPTAP_BSD, DROPTAP_TCP, 26, "TCP bind in progress") \
181 X(DROP_REASON_TCP_MEM_ALLOC, DROPTAP_BSD, DROPTAP_TCP, 27, "TCP memory allocation") \
182 X(DROP_REASON_TCP_PCB_CONNECT, DROPTAP_BSD, DROPTAP_TCP, 28, "TCP protocol control block connect") \
183 X(DROP_REASON_TCP_SYN_RECEIVED_BAD_ACK, DROPTAP_BSD, DROPTAP_TCP, 29, "TCP SYN_RECEIVED bad ACK") \
184 X(DROP_REASON_TCP_SYN_SENT_BAD_ACK, DROPTAP_BSD, DROPTAP_TCP, 30, "TCP SYN_SENT bad ACK") \
185 X(DROP_REASON_TCP_SYN_SENT_NO_SYN, DROPTAP_BSD, DROPTAP_TCP, 31, "TCP SYN_SENT no SYN") \
186 X(DROP_REASON_TCP_ACK_TOOMUCH, DROPTAP_BSD, DROPTAP_TCP, 32, "TCP ACK rate limit") \
187 X(DROP_REASON_TCP_OLD_ACK, DROPTAP_BSD, DROPTAP_TCP, 33, "TCP challenge ACK") \
188 X(DROP_REASON_TCP_SYN_DATA_INVALID, DROPTAP_BSD, DROPTAP_TCP, 34, "TCP SYN data invalid") \
189 X(DROP_REASON_TCP_SYN_RECEIVED_BAD_SEQ, DROPTAP_BSD, DROPTAP_TCP, 35, "TCP SYN_RECEIVED bad sequence number") \
190 X(DROP_REASON_TCP_RECV_AFTER_CLOSE, DROPTAP_BSD, DROPTAP_TCP, 36, "TCP receive after close") \
191 X(DROP_REASON_TCP_BAD_ACK, DROPTAP_BSD, DROPTAP_TCP, 37, "TCP bad ACK") \
192 X(DROP_REASON_TCP_BAD_RST, DROPTAP_BSD, DROPTAP_TCP, 38, "TCP bad RST") \
193 X(DROP_REASON_TCP_PAWS, DROPTAP_BSD, DROPTAP_TCP, 39, "TCP PAWS") \
194 X(DROP_REASON_TCP_REASS_MEMORY_PRESSURE, DROPTAP_BSD, DROPTAP_TCP, 40, "TCP reassembly queue memory pressure") \
195 X(DROP_REASON_TCP_CREATE_SERVER_SOCKET, DROPTAP_BSD, DROPTAP_TCP, 41, "TCP create server socket failed") \
196 X(DROP_REASON_TCP_INSEQ_MEMORY_PRESSURE, DROPTAP_BSD, DROPTAP_TCP, 42, "TCP in-seq input under memory pressure") \
197 /* IP */ \
198 X(DROP_REASON_IP_UNKNOWN_MULTICAST_GROUP, DROPTAP_BSD, DROPTAP_IP, 2, "IP unknown multicast group join") \
199 X(DROP_REASON_IP_INVALID_ADDR, DROPTAP_BSD, DROPTAP_IP, 3, "Invalid IP address") \
200 X(DROP_REASON_IP_TOO_SHORT, DROPTAP_BSD, DROPTAP_IP, 4, "IP packet too short") \
201 X(DROP_REASON_IP_TOO_SMALL, DROPTAP_BSD, DROPTAP_IP, 5, "IP header too small") \
202 X(DROP_REASON_IP_RCV_IF_NO_MATCH, DROPTAP_BSD, DROPTAP_IP, 6, "IP receive interface no match") \
203 X(DROP_REASON_IP_CANNOT_FORWARD, DROPTAP_BSD, DROPTAP_IP, 7, "IP cannot forward") \
204 X(DROP_REASON_IP_BAD_VERSION, DROPTAP_BSD, DROPTAP_IP, 8, "IP bad version") \
205 X(DROP_REASON_IP_BAD_CHECKSUM, DROPTAP_BSD, DROPTAP_IP, 9, "IP bad checksum") \
206 X(DROP_REASON_IP_BAD_HDR_LENGTH, DROPTAP_BSD, DROPTAP_IP, 10, "IP bad header length") \
207 X(DROP_REASON_IP_BAD_LENGTH, DROPTAP_BSD, DROPTAP_IP, 11, "IP bad length") \
208 X(DROP_REASON_IP_BAD_TTL, DROPTAP_BSD, DROPTAP_IP, 12, "IP bad TTL") \
209 X(DROP_REASON_IP_NO_PROTO, DROPTAP_BSD, DROPTAP_IP, 13, "IP unknown protocol") \
210 X(DROP_REASON_IP_FRAG_NOT_ACCEPTED, DROPTAP_BSD, DROPTAP_IP, 14, "IP fragment not accepted") \
211 X(DROP_REASON_IP_FRAG_DROPPED, DROPTAP_BSD, DROPTAP_IP, 15, "IP fragment dropped") \
212 X(DROP_REASON_IP_FRAG_TIMEOUT, DROPTAP_BSD, DROPTAP_IP, 16, "IP fragment timeout") \
213 X(DROP_REASON_IP_FRAG_TOO_MANY, DROPTAP_BSD, DROPTAP_IP, 17, "IP fragment too many") \
214 X(DROP_REASON_IP_FRAG_TOO_LONG, DROPTAP_BSD, DROPTAP_IP, 18, "IP fragment too long") \
215 X(DROP_REASON_IP_FRAG_DRAINED, DROPTAP_BSD, DROPTAP_IP, 19, "IP fragment drained") \
216 X(DROP_REASON_IP_FILTER_DROP, DROPTAP_BSD, DROPTAP_IP, 20, "IP filter drop") \
217 X(DROP_REASON_IP_FRAG_TOO_SMALL, DROPTAP_BSD, DROPTAP_IP, 21, "IP too small to fragment") \
218 X(DROP_REASON_IP_FRAG_NO_MEM, DROPTAP_BSD, DROPTAP_IP, 22, "IP no memory for fragmentation") \
219 X(DROP_REASON_IP_CANNOT_FRAGMENT, DROPTAP_BSD, DROPTAP_IP, 23, "IP cannot fragment") \
220 X(DROP_REASON_IP_OUTBOUND_IPSEC_POLICY, DROPTAP_BSD, DROPTAP_IP, 24, "IP outbound IPsec policy") \
221 X(DROP_REASON_IP_ZERO_NET, DROPTAP_BSD, DROPTAP_IP, 25, "IP to network zero") \
222 X(DROP_REASON_IP_SRC_ADDR_NO_AVAIL, DROPTAP_BSD, DROPTAP_IP, 26, "IP source address not available") \
223 X(DROP_REASON_IP_DST_ADDR_NO_AVAIL, DROPTAP_BSD, DROPTAP_IP, 27, "IP destination address not available") \
224 X(DROP_REASON_IP_TO_RESTRICTED_IF, DROPTAP_BSD, DROPTAP_IP, 28, "IP packet to a restricted interface") \
225 X(DROP_REASON_IP_NO_ROUTE, DROPTAP_BSD, DROPTAP_IP, 29, "IP no route") \
226 X(DROP_REASON_IP_IF_CANNOT_MULTICAST, DROPTAP_BSD, DROPTAP_IP, 30, "IP multicast not supported by interface") \
227 X(DROP_REASON_IP_SRC_ADDR_ANY, DROPTAP_BSD, DROPTAP_IP, 31, "IP source address any") \
228 X(DROP_REASON_IP_IF_CANNOT_BROADCAST, DROPTAP_BSD, DROPTAP_IP, 32, "IP broadcast not supported by interface") \
229 X(DROP_REASON_IP_BROADCAST_NOT_ALLOWED, DROPTAP_BSD, DROPTAP_IP, 33, "IP broadcast not allowed") \
230 X(DROP_REASON_IP_BROADCAST_TOO_BIG, DROPTAP_BSD, DROPTAP_IP, 34, "IP broadcast too big for MTU") \
231 X(DROP_REASON_IP_FILTER_TSO, DROPTAP_BSD, DROPTAP_IP, 35, "TSO packet to IP filter") \
232 X(DROP_REASON_IP_NECP_POLICY_NO_ALLOW_IF, DROPTAP_BSD, DROPTAP_IP, 36, "NECP not allowed on interface") \
233 X(DROP_REASON_IP_NECP_POLICY_DROP, DROPTAP_BSD, DROPTAP_IP, 37, "NECP drop") \
234 X(DROP_REASON_IP_NECP_POLICY_SOCKET_DIVERT, DROPTAP_BSD, DROPTAP_IP, 38, "NECP socket divert") \
235 X(DROP_REASON_IP_NECP_POLICY_TUN_NO_ALLOW_IF, DROPTAP_BSD, DROPTAP_IP, 39, "NECP tunnel not allowed on interface") \
236 X(DROP_REASON_IP_NECP_POLICY_TUN_REBIND_NO_ALLOW_IF, DROPTAP_BSD, DROPTAP_IP, 40, "NECP rebind not allowed on interface") \
237 X(DROP_REASON_IP_NECP_POLICY_TUN_NO_REBIND_IF, DROPTAP_BSD, DROPTAP_IP, 41, "NECP rebind not allowed on interface") \
238 X(DROP_REASON_IP_NECP_NO_ALLOW_IF, DROPTAP_BSD, DROPTAP_IP, 42, "NECP packet not allowed on interface") \
239 X(DROP_REASON_IP_ENOBUFS, DROPTAP_BSD, DROPTAP_IP, 43, "IP No buffer space available") \
240 X(DROP_REASON_IP_ILLEGAL_PORT, DROPTAP_BSD, DROPTAP_IP, 44, "IP Illegal port") \
241 X(DROP_REASON_IP_UNREACHABLE_PORT, DROPTAP_BSD, DROPTAP_IP, 45, "IP Unreachable port") \
242 X(DROP_REASON_IP_MULTICAST_NO_PORT, DROPTAP_BSD, DROPTAP_IP, 46, "IP Multicast no port") \
243 X(DROP_REASON_IP_EISCONN, DROPTAP_BSD, DROPTAP_IP, 47, "IP Socket is already connected") \
244 X(DROP_REASON_IP_EAFNOSUPPORT, DROPTAP_BSD, DROPTAP_IP, 48, "IP Address family not supported by protocol family") \
245 X(DROP_REASON_IP_NO_SOCK, DROPTAP_BSD, DROPTAP_IP, 49, "IP No matching sock") \
246 /* IPsec */ \
247 X(DROP_REASON_IPSEC_REJECT, DROPTAP_BSD, DROPTAP_IPSEC,1, "IPsec reject") \
248 /* IPv6 */ \
249 X(DROP_REASON_IP6_OPT_DISCARD, DROPTAP_BSD, DROPTAP_IP6, 1, "IPv6 discard option") \
250 X(DROP_REASON_IP6_IF_IPV6_DISABLED, DROPTAP_BSD, DROPTAP_IP6, 2, "IPv6 is disabled on the interface") \
251 X(DROP_REASON_IP6_BAD_SCOPE, DROPTAP_BSD, DROPTAP_IP6, 3, "IPv6 bad scope") \
252 X(DROP_REASON_IP6_UNPROXIED_NS, DROPTAP_BSD, DROPTAP_IP6, 4, "IPv6 unproxied mistargeted Neighbor Solicitation") \
253 X(DROP_REASON_IP6_BAD_OPTION, DROPTAP_BSD, DROPTAP_IP6, 5, "IPv6 bad option") \
254 X(DROP_REASON_IP6_TOO_MANY_OPTIONS, DROPTAP_BSD, DROPTAP_IP6, 6, "IPv6 too many header options") \
255 X(DROP_REASON_IP6_BAD_PATH_MTU, DROPTAP_BSD, DROPTAP_IP6, 7, "IPv6 bad path MTU") \
256 X(DROP_REASON_IP6_NO_PREFERRED_SRC_ADDR, DROPTAP_BSD, DROPTAP_IP6, 8, "IPv6 no preferred source address") \
257 X(DROP_REASON_IP6_BAD_HLIM, DROPTAP_BSD, DROPTAP_IP6, 9, "IPv6 bad HLIM") \
258 X(DROP_REASON_IP6_BAD_DAD, DROPTAP_BSD, DROPTAP_IP6, 10, "IPv6 bad DAD") \
259 X(DROP_REASON_IP6_NO_ND6ALT_IF, DROPTAP_BSD, DROPTAP_IP6, 11, "IPv6 no ND6ALT interface") \
260 X(DROP_REASON_IP6_BAD_ND_STATE, DROPTAP_BSD, DROPTAP_IP6, 12, "IPv6 Bad ND state") \
261 X(DROP_REASON_IP6_ONLY, DROPTAP_BSD, DROPTAP_IP6, 13, "IPv6 Only") \
262 X(DROP_REASON_IP6_ADDR_UNSPECIFIED, DROPTAP_BSD, DROPTAP_IP6, 14, "IPv6 Address is unspecified") \
263 X(DROP_REASON_IP6_FRAG_OVERLAPPING, DROPTAP_BSD, DROPTAP_IP6, 15, "IPv6 Fragment overlaping") \
264 X(DROP_REASON_IP6_FRAG_MIXED_CE, DROPTAP_BSD, DROPTAP_IP6, 16, "IPv6 Fragment mixed CE bits") \
265 X(DROP_REASON_IP6_RA_NOT_LL, DROPTAP_BSD, DROPTAP_IP6, 17, "IPv6 RA src is not LL") \
266 X(DROP_REASON_IP6_RA_BAD_LLADDR_LEN, DROPTAP_BSD, DROPTAP_IP6, 18, "IPv6 RA bad LL length") \
267 X(DROP_REASON_IP6_RS_BAD_LLADDR_LEN, DROPTAP_BSD, DROPTAP_IP6, 19, "IPv6 RS bad LL length") \
268 X(DROP_REASON_IP6_MEM_ALLOC, DROPTAP_BSD, DROPTAP_IP6, 20, "IPv6 memory allocation") \
269 X(DROP_REASON_IP6_TOO_BIG, DROPTAP_BSD, DROPTAP_IP6, 21, "IPv6 too big for MTU") \
270 X(DROP_REASON_IP6_POSSIBLE_LOOP, DROPTAP_BSD, DROPTAP_IP6, 22, "IPv6 possible loop") \
271 X(DROP_REASON_IP6_ICMP_DROP, DROPTAP_BSD, DROPTAP_IP6, 23, "IPv6 ICMPv6 drop") \
272 X(DROP_REASON_IP6_BAD_NI, DROPTAP_BSD, DROPTAP_IP6, 24, "IPv6 bad NI") \
273 X(DROP_REASON_IP6_NS_FROM_NON_NEIGHBOR, DROPTAP_BSD, DROPTAP_IP6, 25, "IPv6 NS from non-neighbor") \
274 X(DROP_REASON_IP6_NS_TO_MULTICAST, DROPTAP_BSD, DROPTAP_IP6, 26, "IPv6 NS targeting multicast") \
275 X(DROP_REASON_IP6_NS_BAD_ND_OPT, DROPTAP_BSD, DROPTAP_IP6, 27, "IPv6 NS with invalid ND opt") \
276 X(DROP_REASON_IP6_NS_BAD_LLADDR_LEN, DROPTAP_BSD, DROPTAP_IP6, 28, "IPv6 NS bad LL length") \
277 X(DROP_REASON_IP6_NS_DUPLICATE_ADDRESS, DROPTAP_BSD, DROPTAP_IP6, 29, "IPv6 NS duplicate address") \
278 X(DROP_REASON_IP6_NS_INVALID_TARGET, DROPTAP_BSD, DROPTAP_IP6, 30, "IPv6 NS invalid target") \
279 X(DROP_REASON_IP6_NA_INVALID_TARGET, DROPTAP_BSD, DROPTAP_IP6, 31, "IPv6 NA invalid target") \
280 X(DROP_REASON_IP6_NA_DST_MULTICAST, DROPTAP_BSD, DROPTAP_IP6, 32, "IPv6 NA destination is multicast") \
281 X(DROP_REASON_IP6_NA_UNKNOWN_SRC_ADDR, DROPTAP_BSD, DROPTAP_IP6, 33, "IPv6 NA destination is multicast") \
282 X(DROP_REASON_IP6_NA_BAD_LLADDR_LEN, DROPTAP_BSD, DROPTAP_IP6, 34, "IPv6 NA bad LL length") \
283 X(DROP_REASON_IP6_NA_NOT_CACHED_SCOPED, DROPTAP_BSD, DROPTAP_IP6, 35, "IPv6 NA not cached scoped ") \
284 X(DROP_REASON_IP6_NA_NOT_CACHED, DROPTAP_BSD, DROPTAP_IP6, 36, "IPv6 NA not cached") \
285 X(DROP_REASON_IP6_NA_MISSING_LLADDR_OPT, DROPTAP_BSD, DROPTAP_IP6, 37, "IPv6 NA missing lladdr opt") \
286 X(DROP_REASON_IP6_NA_MISSING_ROUTE, DROPTAP_BSD, DROPTAP_IP6, 38, "IPv6 NA missing route info") \
287 X(DROP_REASON_IP6_BAD_UDP_CHECKSUM, DROPTAP_BSD, DROPTAP_IP6, 39, "IPv6 invalid UDP checksum") \
288 X(DROP_REASON_IP6_ILLEGAL_PORT, DROPTAP_BSD, DROPTAP_IP6, 40, "IPv6 Illegal port") \
289 /* UDP */ \
290 X(DROP_REASON_UDP_SET_PORT_FAILURE, DROPTAP_BSD, DROPTAP_UDP, 1, "UDP failed to set ephemeral port ") \
291 X(DROP_REASON_UDP_DST_PORT_ZERO, DROPTAP_BSD, DROPTAP_UDP, 2, "UDP destination port zero") \
292 X(DROP_REASON_UDP_BAD_LENGTH, DROPTAP_BSD, DROPTAP_UDP, 3, "UDP bad length") \
293 X(DROP_REASON_UDP_BAD_CHECKSUM, DROPTAP_BSD, DROPTAP_UDP, 4, "UDP bad checksum") \
294 X(DROP_REASON_UDP_PORT_UNREACHEABLE, DROPTAP_BSD, DROPTAP_UDP, 5, "UDP port unreachable") \
295 X(DROP_REASON_UDP_SOCKET_CLOSING, DROPTAP_BSD, DROPTAP_UDP, 6, "UDP socket closing") \
296 X(DROP_REASON_UDP_NECP, DROPTAP_BSD, DROPTAP_UDP, 7, "UDP denied by NECP") \
297 X(DROP_REASON_UDP_CANNOT_SAVE_CONTROL, DROPTAP_BSD, DROPTAP_UDP, 8, "UDP cannot save control mbufs") \
298 X(DROP_REASON_UDP_IPSEC, DROPTAP_BSD, DROPTAP_UDP, 9, "UDP IPsec") \
299 X(DROP_REASON_UDP_PACKET_SHORTER_THAN_HEADER, DROPTAP_BSD, DROPTAP_UDP, 10, "UDP packet shorter than header") \
300 X(DROP_REASON_UDP_NAT_KEEPALIVE, DROPTAP_BSD, DROPTAP_UDP, 11, "UDP NAT keepalive") \
301 X(DROP_REASON_UDP_PCB_GARBAGE_COLLECTED, DROPTAP_BSD, DROPTAP_UDP, 12, "UDP PCB garbage collected") \
302
303
304#endif /* PACKET_DARWIN_DROPTAP_MSG_H */