| Wireshark 4.7.0 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
DTM_Dynamic_Allocation_t Struct Reference

## Public Attributes
uint8_t | Extended_Dynamic_Allocation
uint8_t | Exist_P0
uint8_t | P0
uint8_t | PR_MODE
uint8_t | USF_GRANULARITY
uint8_t | Exist_UPLINK_TFI_ASSIGNMENT
uint8_t | UPLINK_TFI_ASSIGNMENT
uint8_t | Exist_RLC_DATA_BLOCKS_GRANTED
uint8_t | RLC_DATA_BLOCKS_GRANTED
uint8_t | UnionType
union { |
Timeslot_Allocation_t Timeslot_Allocation [8] |
Timeslot_Allocation_Power_Ctrl_Param_t Timeslot_Allocation_Power_Ctrl_Param |
} | u |

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/epan/dissectors/packet-gsm_rlcmac.h