| Wireshark 4.7.0 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
_h323_calls_info Struct Reference

`#include <voip_calls.h>`

## Public Attributes
e_guid_t * | guid
GList * | h245_list
address | h225SetupAddr
bool | is_h245
bool | is_faststart_Setup
bool | is_faststart_Proc
bool | is_h245Tunneling
int32_t | q931_crv
int32_t | q931_crv2
unsigned | requestSeqNum

## Detailed Description

defines specific H323 data

## Member Data Documentation

## ◆ h225SetupAddr

address _h323_calls_info::h225SetupAddr

we use the SETUP H225 IP to determine if packets are forward or reverse

## ◆ h245_list

GList* _h323_calls_info::h245_list

list of H245 Address and ports for tunneling off calls

## ◆ is_faststart_Proc

bool _h323_calls_info::is_faststart_Proc

if faststart field is included in Proce, Alerting, Progress or Connect

## ◆ is_faststart_Setup

bool _h323_calls_info::is_faststart_Setup

if faststart field is included in Setup

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/ui/voip_calls.h