| Wireshark 4.7.0 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
Multislot_capability_t Struct Reference

## Public Attributes
uint8_t | Exist_HSCSD_multislot_class
uint8_t | HSCSD_multislot_class
uint8_t | Exist_GPRS_multislot_class
uint8_t | GPRS_multislot_class
uint8_t | GPRS_Extended_Dynamic_Allocation_Capability
uint8_t | Exist_SM
uint8_t | SMS_VALUE
uint8_t | SM_VALUE
uint8_t | Exist_ECSD_multislot_class
uint8_t | ECSD_multislot_class
uint8_t | Exist_EGPRS_multislot_class
uint8_t | EGPRS_multislot_class
uint8_t | EGPRS_Extended_Dynamic_Allocation_Capability
uint8_t | Exist_DTM_GPRS_multislot_class
uint8_t | DTM_GPRS_multislot_class
uint8_t | Single_Slot_DTM
DTM_EGPRS_t | DTM_EGPRS_Params

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/epan/dissectors/packet-gsm_rlcmac.h