| Wireshark 4.7.0 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
media_description_t Struct Reference

## Public Attributes
transport_proto_t | proto
uint32_t | media_types
bool | bundled
uint16_t | media_port
uint16_t | control_port
address | conn_addr
char * | control_uri
transport_media_pt_t | media
union { |
struct { |
address ipaddr |
uint16_t port_number |
} msrp |
} | media_attr |

## Member Data Documentation

## ◆ bundled

bool media_description_t::bundled

"m=" lines are "bundled", that is, all on same port

## ◆ conn_addr

address media_description_t::conn_addr

The address from the "c=" line (default from session level, possibly overridden at the media level).

## ◆ control_port

uint16_t media_description_t::control_port

Port number, parsed from "a=rtcp" or "a=rtcp-mux" line.

## ◆ control_uri

char* media_description_t::control_uri

RTSP media control URI, parsed from "a=control:" XXX - allowed to default to session level if not overridden if only one media desc, but this is not implemented yet.

## ◆ media

transport_media_pt_t media_description_t::media

Information about payload numbers for this media.

## ◆ media_port

uint16_t media_description_t::media_port

Port number, parsed from "m=" line.

## ◆ media_types

uint32_t media_description_t::media_types

Whether "m=video" or others

## ◆ [struct]

struct { ... } media_description_t::msrp

MSRP transport info, parsed from "a=label:"

## ◆ proto

transport_proto_t media_description_t::proto

Protocol, parsed from "m=" line.

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/epan/dissectors/packet-sdp.c