| Wireshark 4.7.0 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
tap-iax2-analysis.h
Go to the documentation of this file.
1
20#ifndef __TAP_IAX2_ANALYSIS_H__
21#define __TAP_IAX2_ANALYSIS_H__
22
23#include <epan/address.h>
24#include <epan/packet_info.h>
25
31#ifdef __cplusplus
32 extern "C" {
33#endif /* __cplusplus */
34
35/****************************************************************************/
36/* structure that holds the information about the forward and reversed direction */
37 typedef struct _iax2_bw_history_item {
38 double time;
39 uint32_t bytes;
40} iax2_bw_history_item;
41
42#define BUFF_BW 300
43
44 typedef struct _tap_iax2_stat_t {
45 bool first_packet; /* do not use in code that is called after iax2_packet_analyse */
46 /* use (flags & STAT_FLAG_FIRST) instead */
47 /* all of the following fields will be initialized after
48 iax2_packet_analyse has been called */
49 uint32_t flags; /* see STAT_FLAG-defines below */
50 uint16_t seq_num;
51 uint32_t timestamp;
52 uint32_t delta_timestamp;
53 double bandwidth;
54 iax2_bw_history_item bw_history[BUFF_BW];
55 uint16_t bw_start_index;
56 uint16_t bw_index;
57 uint32_t total_bytes;
58 double delta;
59 double jitter;
60 double diff;
61 double time;
62 double start_time;
63 double max_delta;
64 double max_jitter;
65 double mean_jitter;
66 uint32_t max_nr;
67 uint16_t start_seq_nr;
68 uint16_t stop_seq_nr;
69 uint32_t total_nr;
70 uint32_t sequence;
71 bool under; /* Unused? */
72 int cycles; /* Unused? */
73 uint16_t pt;
74 int reg_pt;
75} tap_iax2_stat_t;
76
77#define PT_UNDEFINED -1
78
79/* status flags for the flags parameter in tap_iax2_stat_t */
80#define STAT_FLAG_FIRST 0x001
81#define STAT_FLAG_MARKER 0x002
82#define STAT_FLAG_WRONG_SEQ 0x004
83#define STAT_FLAG_PT_CHANGE 0x008
84#define STAT_FLAG_PT_CN 0x010
85#define STAT_FLAG_FOLLOW_PT_CN 0x020
86#define STAT_FLAG_REG_PT_CHANGE 0x040
87#define STAT_FLAG_WRONG_TIMESTAMP 0x080
88
89/* function for analysing an IAX2 packet. Called from iax2_analysis. */
90 extern void iax2_packet_analyse(tap_iax2_stat_t *statinfo,
91 packet_info *pinfo,
92 const struct _iax2_info_t *iax2info);
93
94#ifdef __cplusplus
95}
96#endif /* __cplusplus */
97
98#endif /* __TAP_IAX2_ANALYSIS_H__ */
address.h
packet_info.h
_iax2_bw_history_item
Definition tap-iax2-analysis.h:37
_iax2_info_t
Definition packet-iax2.h:294
_packet_info
Definition packet_info.h:43
_tap_iax2_stat_t
Definition tap-iax2-analysis.h:44