| Wireshark 4.7.0 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
ipproto.h
Go to the documentation of this file.
1
12#ifndef __IPPROTO_H__
13#define __IPPROTO_H__
14
15#include "ws_symbol_export.h"
16#include <wsutil/value_string.h>
17
18/*
19 * IP protocol numbers.
20 * http://www.iana.org/assignments/protocol-numbers/protocol-numbers.xml
21 */
22#define IP_PROTO_HOPOPTS 0 /* IP6 hop-by-hop options - RFC1883 */
23#define IP_PROTO_ICMP 1 /* control message protocol - RFC792 */
24#define IP_PROTO_IGMP 2 /* group mgmt protocol - RFC1112 */
25#define IP_PROTO_GGP 3 /* gateway^2 (deprecated) - RFC823*/
26#define IP_PROTO_IPIP 4 /* IP inside IP - RFC2003*/
27#define IP_PROTO_IPV4 4 /* IP header */
28#define IP_PROTO_STREAM 5 /* Stream - RFC1190, RFC1819 */
29#define IP_PROTO_TCP 6 /* TCP - RFC792 */
30#define IP_PROTO_CBT 7 /* CBT - <A.Ballardie@cs.ucl.ac.uk> */
31#define IP_PROTO_EGP 8 /* exterior gateway protocol - RFC888 */
32#define IP_PROTO_IGP 9 /* any private interior gateway protocol ... */
33#define IP_PROTO_IGRP 9 /* ... and used by Cisco for IGRP */
34#define IP_PROTO_BBN_RCC 10 /* BBN RCC Monitoring */
35#define IP_PROTO_NVPII 11 /* Network Voice Protocol - RFC741 */
36#define IP_PROTO_PUP 12 /* pup */
37#define IP_PROTO_ARGUS 13 /* ARGUS */
38#define IP_PROTO_EMCON 14 /* EMCON */
39#define IP_PROTO_XNET 15 /* Cross net debugger - IEN158 */
40#define IP_PROTO_CHAOS 16 /* CHAOS */
41#define IP_PROTO_UDP 17 /* user datagram protocol - RFC768 */
42#define IP_PROTO_MUX 18 /* multiplexing - IEN90 */
43#define IP_PROTO_DCNMEAS 19 /* DCN Measurement Subsystems */
44#define IP_PROTO_HMP 20 /* Host Monitoring - RFC869 */
45#define IP_PROTO_PRM 21 /* Packet radio measurement */
46#define IP_PROTO_IDP 22 /* xns idp */
47#define IP_PROTO_TRUNK1 23
48#define IP_PROTO_TRUNK2 24
49#define IP_PROTO_LEAF1 25
50#define IP_PROTO_LEAF2 26
51#define IP_PROTO_RDP 27 /* Reliable Data Protocol - RFC908 */
52#define IP_PROTO_IRT 28 /* Internet Reliable Transaction - RFC938 */
53#define IP_PROTO_TP 29 /* tp-4 w/ class negotiation - RFC905 */
54#define IP_PROTO_BULK 30 /* Bulk Data Transfer Protocol - RFC969 */
55#define IP_PROTO_MFE_NSP 31 /* MFE Network Services Protocol */
56#define IP_PROTO_MERIT 32 /* MERIT Internodal Protocol */
57#define IP_PROTO_DCCP 33 /* Datagram Congestion Control Protocol */
58#define IP_PROTO_3PC 34 /* Third party connect protocol */
59#define IP_PROTO_IDPR 35 /* Interdomain policy routing protocol */
60#define IP_PROTO_XTP 36 /* Xpress Transport Protocol */
61#define IP_PROTO_DDP 37 /* Datagram Delivery Protocol */
62#define IP_PROTO_CMTP 38 /* Control Message Transport Protocol */
63#define IP_PROTO_TPPP 39 /* TP++ Transport Protocol */
64#define IP_PROTO_IL 40 /* IL Transport Protocol */
65#define IP_PROTO_IPV6 41 /* IP6 header */
66#define IP_PROTO_SDRP 42 /* Source demand routing protocol */
67#define IP_PROTO_ROUTING 43 /* IP6 routing header */
68#define IP_PROTO_FRAGMENT 44 /* IP6 fragmentation header */
69#define IP_PROTO_IDRP 45 /* Inter-Domain Routing Protocol */
70#define IP_PROTO_RSVP 46 /* Resource ReSerVation protocol */
71#define IP_PROTO_GRE 47 /* General Routing Encapsulation */
72#define IP_PROTO_DSR 48 /* Dynamic Source Routing Protocol */
73#define IP_PROTO_BNA 49 /* BNA */
74#define IP_PROTO_ESP 50 /* Encap Security Payload for IPv6 - RFC2406 */
75#define IP_PROTO_AH 51 /* Authentication Header for IPv6 - RFC2402*/
76#define IP_PROTO_INSLP 52 /* Integrated Net Layer Security */
77#define IP_PROTO_SWIPE 53 /* IP with Encryption */
78#define IP_PROTO_NARP 54 /* NBMA Address resolution protocol - RFC1735 */
79#define IP_PROTO_MOBILE 55 /* IP Mobility */
80#define IP_PROTO_TLSP 56 /* Transport Layer Security Protocol using */
81 /* Kryptonet key management */
82#define IP_PROTO_SKIP 57 /* SKIP */
83#define IP_PROTO_ICMPV6 58 /* ICMP6 - RFC1883*/
84#define IP_PROTO_NONE 59 /* IP6 no next header - RFC1883 */
85#define IP_PROTO_DSTOPTS 60 /* IP6 destination options - RFC1883 */
86/* 61 is reserved by IANA for any host internal protocol */
87
88/*
89 * The current Protocol Numbers list says that the IP protocol number for
90 * mobility headers is 135; it cites draft-ietf-mobileip-ipv6-24, but
91 * that draft doesn't actually give a number.
92 *
93 * It appears that 62 used to be used, even though that's assigned to
94 * a protocol called CFTP; however, the only reference for CFTP is a
95 * Network Message from BBN back in 1982, so, for now, we support 62,
96 * as well as 135, as a protocol number for mobility headers.
97 */
98#define IP_PROTO_MIPV6_OLD 62 /* Mobile IPv6 */
99/* 63 is reserved by IANA for any local network */
100#define IP_PROTO_SATEXPAK 64
101#define IP_PROTO_KRYPTOLAN 65
102#define IP_PROTO_RVD 66 /* MIT Remote virtual disk protocol */
103#define IP_PROTO_IPPC 67 /* Internet Pluribus Packet Core */
104/* 68 is reserved by IANA for any distributed file system */
105#define IP_PROTO_SATMON 69 /* SATNET Monitoring */
106#define IP_PROTO_VISA 70 /* VISA Protocol */
107#define IP_PROTO_IPCV 71 /* Internet Packet Core Utility */
108#define IP_PROTO_CPNX 72 /* Computer Protocol Network Executive */
109#define IP_PROTO_CPHB 73 /* Computer Protocol Heart Beat */
110#define IP_PROTO_WSN 74 /* WANG Span Network */
111#define IP_PROTO_PVP 75 /* Packet Video Protocol */
112#define IP_PROTO_BRSATMON 76 /* Backroom SATNET Monitoring */
113#define IP_PROTO_SUNND 77 /* SUN ND Protocol - Temporary */
114#define IP_PROTO_WBMON 78 /* Wideband Monitoring */
115#define IP_PROTO_WBEXPAK 79 /* Wideband EXPAK */
116#define IP_PROTO_ISOIP 80 /* ISO IP */
117#define IP_PROTO_VMTP 81
118#define IP_PROTO_SVMTP 82 /* Secure VMTP */
119#define IP_PROTO_VINES 83 /* Vines over raw IP */
120#define IP_PROTO_TTP 84
121#define IP_PROTO_NSFNETIGP 85 /* NSFNET IGP */
122#define IP_PROTO_DGP 86 /* Dissimilar Gateway Protocol */
123#define IP_PROTO_TCF 87
124#define IP_PROTO_EIGRP 88
125#define IP_PROTO_OSPF 89 /* OSPF Interior Gateway Protocol - RFC1583 */
126#define IP_PROTO_SPRITE 90 /* SPRITE RPC protocol */
127#define IP_PROTO_LARP 91 /* Locus Address Resolution Protocol */
128#define IP_PROTO_MTP 92 /* Multicast Transport Protocol */
129#define IP_PROTO_AX25 93 /* AX.25 frames */
130#define IP_PROTO_IPINIP 94 /* IP within IP Encapsulation protocol */
131#define IP_PROTO_MICP 95 /* Mobile Internetworking Control Protocol */
132#define IP_PROTO_SCCCP 96 /* Semaphore communications security protocol */
133#define IP_PROTO_ETHERIP 97 /* Ethernet-within-IP - RFC 3378 */
134#define IP_PROTO_ENCAP 98 /* encapsulation header - RFC1241*/
135/* 99 is reserved by IANA for any private encryption scheme */
136#define IP_PROTO_GMTP 100
137#define IP_PROTO_IFMP 101 /* Ipsilon flow management protocol */
138#define IP_PROTO_PNNI 102 /* PNNI over IP */
139#define IP_PROTO_PIM 103 /* Protocol Independent Mcast */
140#define IP_PROTO_ARIS 104
141#define IP_PROTO_SCPS 105
142#define IP_PROTO_QNX 106
143#define IP_PROTO_AN 107 /* Active Networks */
144#define IP_PROTO_IPCOMP 108 /* IP payload compression - RFC2393 */
145#define IP_PROTO_SNP 109 /* Sitara Networks Protocol */
146#define IP_PROTO_COMPAQ 110 /* Compaq Peer Protocol */
147#define IP_PROTO_IPX 111 /* IPX over IP */
148#define IP_PROTO_VRRP 112 /* Virtual Router Redundancy Protocol */
149#define IP_PROTO_PGM 113 /* Pragmatic General Multicast */
150/* 114 is reserved by IANA for any zero hop protocol */
151#define IP_PROTO_L2TP 115 /* Layer Two Tunnelling Protocol */
152#define IP_PROTO_DDX 116 /* D-II Data Exchange */
153#define IP_PROTO_IATP 117 /* Interactive Agent Transfer Protocol */
154#define IP_PROTO_STP 118 /* Schedule Transfer Protocol */
155#define IP_PROTO_SRP 119 /* Spectralink Radio Protocol */
156#define IP_PROTO_UTI 120
157#define IP_PROTO_SMP 121 /* Simple Message Protocol */
158#define IP_PROTO_SM 122
159#define IP_PROTO_PTP 123 /* Performance Transparency Protocol */
160#define IP_PROTO_ISIS 124 /* ISIS over IPv4 */
161#define IP_PROTO_FIRE 125
162#define IP_PROTO_CRTP 126 /* Combat Radio Transport Protocol */
163#define IP_PROTO_CRUDP 127 /* Combat Radio User Datagram */
164#define IP_PROTO_SSCOPMCE 128
165#define IP_PROTO_IPLT 129
166#define IP_PROTO_SPS 130 /* Secure Packet Shield */
167#define IP_PROTO_PIPE 131 /* Private IP Encapsulation within IP */
168#define IP_PROTO_SCTP 132 /* Stream Control Transmission Protocol */
169#define IP_PROTO_FC 133 /* Fibre Channel */
170#define IP_PROTO_RSVPE2EI 134 /* RSVP E2E Ignore - RFC3175 */
171#define IP_PROTO_MIPV6 135 /* Mobile IPv6 */
172#define IP_PROTO_UDPLITE 136 /* Lightweight user datagram protocol - RFC3828 */
173#define IP_PROTO_MPLS_IN_IP 137 /* MPLS in IP - RFC4023 */
174#define IP_PROTO_MANET 138 /* MANET Protocols */
175#define IP_PROTO_HIP 139 /* Host Identity Protocol */
176#define IP_PROTO_SHIM6 140 /* Shim6 Protocol */
177#define IP_PROTO_WESP 141 /* 141 WESP Wrapped Encapsulating Security Payload [RFC5840] */
178#define IP_PROTO_ROHC 142 /* 142 ROHC Robust Header Compression [RFC5858] */
179#define IP_PROTO_ETHERNET 143 /* Ethernet [RFC8986] */
180#define IP_PROTO_AGGFRAG 144 /* AGGFRAG encapsulation payload for ESP */
181#define IP_PROTO_NSH 145 /* Network Service Header */
182#define IP_PROTO_HOMA 146 /* Homa */
183#define IP_PROTO_BIT_EMU 147 /* Bit-stream Emulation */
184#define IP_PROTO_AX4000 173 /* AX/4000 Testblock - non IANA */
185#define IP_PROTO_NCS_HEARTBEAT 224 /* Novell NCS Heartbeat - http://support.novell.com/cgi-bin/search/searchtid.cgi?/10071158.htm */
186
187WS_DLL_PUBLIC value_string_ext ipproto_val_ext;
188WS_DLL_PUBLIC const char *ipprotostr(const int proto);
189
190WS_DLL_PUBLIC const char *ipv6extprotostr(int proto);
191
192#endif /* ipproto.h */
193
194/*
195 * Editor modelines
196 *
197 * Local Variables:
198 * c-basic-offset: 4
199 * tab-width: 8
200 * indent-tabs-mode: nil
201 * End:
202 *
203 * ex: set shiftwidth=4 tabstop=8 expandtab:
204 * :indentSize=4:tabSize=8:noTabs=true:
205 */
_value_string_ext
Extended metadata for a value_string array.
Definition value_string.h:325
value_string.h