| Wireshark 4.7.0 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
Public Attributes | List of all members
_e_addr_resolve Struct Reference

Flags to control name resolution. More...

`#include <addr_resolv.h>`

## Public Attributes
bool | mac_name
bool | network_name
bool | transport_name
bool | dns_pkt_addr_resolution
bool | handshake_sni_addr_resolution
bool | use_external_net_name_resolver
bool | vlan_name
bool | ss7pc_name
bool | maxmind_geoip

## Detailed Description

Flags to control name resolution.

## Member Data Documentation

## ◆ dns_pkt_addr_resolution

bool _e_addr_resolve::dns_pkt_addr_resolution

Whether to resolve addresses using captured DNS packets

## ◆ handshake_sni_addr_resolution

bool _e_addr_resolve::handshake_sni_addr_resolution

Whether to resolve addresses using SNI information found in captured handshake packets

## ◆ mac_name

bool _e_addr_resolve::mac_name

Whether to resolve Ethernet MAC to manufacturer names

## ◆ maxmind_geoip

bool _e_addr_resolve::maxmind_geoip

Whether to lookup geolocation information with mmdbresolve

## ◆ network_name

bool _e_addr_resolve::network_name

Whether to resolve IPv4, IPv6, and IPX addresses into host names

## ◆ ss7pc_name

bool _e_addr_resolve::ss7pc_name

Whether to resolve SS7 Point Codes to names

## ◆ transport_name

bool _e_addr_resolve::transport_name

Whether to resolve TCP/UDP/DCCP/SCTP ports into service names

## ◆ use_external_net_name_resolver

bool _e_addr_resolve::use_external_net_name_resolver

Whether to system's configured DNS server to resolve names

## ◆ vlan_name

bool _e_addr_resolve::vlan_name

Whether to resolve VLAN IDs to names

The documentation for this struct was generated from the following file:

- /builds/wireshark/wireshark/epan/addr_resolv.h