| Wireshark 4.7.0 The Wireshark network protocol analyzer

Loading...
Searching...
No Matches
packet-fcfzs.h
1/* packet-fcfzs.h
2 *
3 * Wireshark - Network traffic analyzer
4 * By Gerald Combs <gerald@wireshark.org>
5 * Copyright 1998 Gerald Combs
6 *
7 * SPDX-License-Identifier: GPL-2.0-or-later
8 */
9
10#ifndef __PACKET_FCFZS_H_
11#define __PACKET_FCFZS_H_
12
13/* Opcode definitions */
14#define FC_FZS_GZC 0x100
15#define FC_FZS_GEST 0x111
16#define FC_FZS_GZSN 0x112
17#define FC_FZS_GZD 0x113
18#define FC_FZS_GZM 0x114
19#define FC_FZS_GAZS 0x115
20#define FC_FZS_GZS 0x116
21#define FC_FZS_ADZS 0x200
22#define FC_FZS_AZSD 0x201
23#define FC_FZS_AZS 0x202
24#define FC_FZS_DZS 0x203
25#define FC_FZS_AZM 0x204
26#define FC_FZS_AZD 0x205
27#define FC_FZS_RZM 0x300
28#define FC_FZS_RZD 0x301
29#define FC_FZS_RZS 0x302
30
31 static const value_string fc_fzs_opcode_val[] = {
32 {FC_FZS_GZC , "Get Capabilities"},
33 {FC_FZS_GEST , "Get Enforcement State"},
34 {FC_FZS_GZSN , "Get Zone Set List"},
35 {FC_FZS_GZD , "Get Zone List"},
36 {FC_FZS_GZM , "Get Zone Member List"},
37 {FC_FZS_GAZS , "Get Active Zone Set"},
38 {FC_FZS_GZS , "Get Zone Set"},
39 {FC_FZS_ADZS , "Add Zone Set"},
40 {FC_FZS_AZSD , "Activate Zone Set Direct"},
41 {FC_FZS_AZS , "Activate Zone Set"},
42 {FC_FZS_DZS , "Deactivate Zone Set"},
43 {FC_FZS_AZM , "Add Zone Members"},
44 {FC_FZS_AZD , "Add Zone"},
45 {FC_FZS_RZM , "Remove Zone Members"},
46 {FC_FZS_RZD , "Remove Zone"},
47 {FC_FZS_RZS , "Remove Zone Set"},
48 {FCCT_MSG_ACC , "MSG_ACC"},
49 {FCCT_MSG_RJT , "MSG_RJT"},
50 {0, NULL},
51};
52
53/* Reason code explanations */
54#define FC_FZS_RJT_NODETAIL 0x0
55#define FC_FZS_RJT_ZONENOTSUPPORTED 0x1
56#define FC_FZS_RJT_ZSNUNKNOWN 0x10
57#define FC_FZS_RJT_NZSACTIVE 0x11
58#define FC_FZS_RJT_ZONEUNKNOWN 0x12
59#define FC_FZS_RJT_ZONESTATEUNKNOWN 0x13
60#define FC_FZS_RJT_INVLDPLEN 0x14
61#define FC_FZS_RJT_ZSTOOLARGE 0x15
62#define FC_FZS_RJT_DZSFAIL 0x16
63#define FC_FZS_RJT_NOTSUPPORTED 0x17
64#define FC_FZS_RJT_CAPNOTSUPPORTED 0x18
65#define FC_FZS_RJT_ZMIDTYPEUNKNOWN 0x19
66#define FC_FZS_RJT_INVLDZSDEF 0x1A
67
68 static const value_string fc_fzs_rjt_code_val[] = {
69 {FC_FZS_RJT_NODETAIL , "No Additional Explanation"},
70 {FC_FZS_RJT_ZONENOTSUPPORTED , "Zones Not Supported"},
71 {FC_FZS_RJT_ZSNUNKNOWN , "Zone Set Name Unknown"},
72 {FC_FZS_RJT_NZSACTIVE , "No Zone Set Active"},
73 {FC_FZS_RJT_ZONEUNKNOWN , "Zone Name Unknown"},
74 {FC_FZS_RJT_ZONESTATEUNKNOWN , "Zone State Unknown"},
75 {FC_FZS_RJT_INVLDPLEN , "Incorrect Payload Length"},
76 {FC_FZS_RJT_ZSTOOLARGE , "Zone Set to be Activated Too Large"},
77 {FC_FZS_RJT_DZSFAIL , "Deactivate Zone Set Failed"},
78 {FC_FZS_RJT_NOTSUPPORTED , "Request Not Supported"},
79 {FC_FZS_RJT_CAPNOTSUPPORTED , "Capability Not Supported"},
80 {FC_FZS_RJT_ZMIDTYPEUNKNOWN , "Zone Member Identifier Type Not Supported"},
81 {FC_FZS_RJT_INVLDZSDEF , "Invalid Zone Set Definition"},
82 {0, NULL},
83};
84
85/* Zone Member Identifier Types */
86
87#define FC_FZS_ZONEMBR_PWWN 1
88#define FC_FZS_ZONEMBR_DP 2
89#define FC_FZS_ZONEMBR_FCID 3
90#define FC_FZS_ZONEMBR_NWWN 4
91#define FC_FZS_ZONEMBR_PWWN_LUN 0xE1
92#define FC_FZS_ZONEMBR_DP_LUN 0xE2
93#define FC_FZS_ZONEMBR_FCID_LUN 0xE3
94
95 static const value_string fc_fzs_zonembr_type_val[] = {
96 {0, "Reserved"},
97 {FC_FZS_ZONEMBR_PWWN, "N_Port WWN"},
98 {FC_FZS_ZONEMBR_DP, "Domain/Physical Port (0x00ddpppp)"},
99 {FC_FZS_ZONEMBR_FCID, "FC Address"},
100 {FC_FZS_ZONEMBR_NWWN, "Node WWN"},
101 {FC_FZS_ZONEMBR_PWWN_LUN, "N_Port WWN+LUN"},
102 {FC_FZS_ZONEMBR_DP_LUN, "Domain/Physical Port+LUN"},
103 {FC_FZS_ZONEMBR_FCID_LUN, "FC Address+LUN"},
104 {0, NULL},
105};
106
107#endif
_value_string
Mapping between a 32-bit integer value and its string representation.
Definition value_string.h:33